Instructions on setting up my code

Unzip the zip file

Open the code in visual studio

When the application is running the first thing it checks is for the smart reader, a message box will appear telling you to insert the smart card reader.

When all the fields are filled the save button will work

You must use the USB card reader (smart card reader) to get the UID of the Tag.

The test data in the myNFCdb.sql (which is in the database folder) is put in mainly but tested using the equipment.

Text

Description automatically generated

Graphical user interface, text, application, chat or text message

Description automatically generated

Connection to the server for the data.

Use the table below to identify what tag type you are using, if any of the NFC material you are using isn’t in it then use a NFC Tools on the google app store to find out the manufacturer.

